# Shower Faucet – AGLY10

### Product Description

- Model: AGLY10
- Material: SUS304 stainless steel
- Workmanship: Precision casting
- Installation Type: Wall Mounted
- Surface Treatment: Brushed
- Valve Core Material: Ceramic
- Cartridge: HearT (German)
- Aerator: NEOPERL (Switzerland)
- Handle: Single handle
- Working mode: handheld shower
- Function: Hot and cold mixer
- OEM&ODM: Acceptable
- Spray Type: Normal
Usage: Bathroom shower Faucet[/tw_list_item]
- Warranty: Five years

Parameter

Testing Pressure: 1.6±0.05Mpa (60±5s)
Working Pressure: 0.05Mpa – 1.0Mpa
Working Temperature: 0 – 95 degrees
Maximum flow rate: 2.5 gpm for hand-held shower head

Payment term

-T/T: 30% deposit upon approval of sample, remaining 70% before shipment
-L/C: irrevocable or L/C at sight

Lead time

-1*20GP loading 1800pcs for 30 days
-1*40GP loading 2600pcs for 40 days
-1/40HQ loading 3000pcs for 45 days

Packing

-How to pack: high quality non-woven bag packing with craft box
-The packing can be changed as customer’s requirement

Send Enquiry
Stainless Steel Bathroom Faucet

### Related products

VIEW DETAILS

## Shower Faucet – AGLY02

VIEW DETAILS

## Shower Faucet – AGLY12

VIEW DETAILS

## Shower Faucet – AGLY15

VIEW DETAILS

## Shower Faucet – AGLY08

Translate »