# Lavatory Faucet - AGLP06

### Product Description

- Model: AGLP06
- Material: SUS304 stainless steel
- Workmanship: Precision casting
- Installation Type: Deck Mounted
- Surface Treatment: Brushed
- Valve Core Material: Ceramic
- Cartridge: HearT (German)
- Aerator: NEOPERL (Switzerland)
- Handle: Single handle
- Hole count: one
- Function: Hot and cold mixer
- OEM&ODM: Acceptable
- Spray Type: Normal
- Usage: lavatory faucet
- Warranty: Five years

Parameter

Testing Pressure: 1.6±0.05Mpa (60±5s)
Working Pressure: 0.05Mpa – 1.0Mpa
Working Temperature: 0 – 95 degrees
Maximum flow rate: 2.2 gallons per minute

Payment term

-T/T: 30% deposit upon approval of sample, remaining 70% before shipment
-L/C: irrevocable or L/C at sight

Lead time

-1*20GP loading 2800pcs for 30 days
-1*40GP loading 5000pcs for 40 days
-1/40HQ loading 5200pcs for 45 days

Packing

-How to pack: high quality non-woven bag packing with craft box
-Spare parts: 60cm stainless steel knitted hose, O-ring, fixed gasket, stainless steel installation base
-Inner box size: 340*220*80mm
-outer carton size: 500*460*440mm (14pcs/carton)
-The packing can be changed as customer’s requirement

Send Enquiry
Stainless Steel Basin Faucet

### Related products

VIEW DETAILS

## Basin Faucet – AGLP15

VIEW DETAILS

## Basin Faucet – AGLP16

VIEW DETAILS

## Basin Faucet – AGLP09

VIEW DETAILS

## Basin Faucet – AGLP08

Translate »